;==================
;GSD file for
;Product : IND570 Industrial Terminal
;Manufacturer: Mettler-Toledo, LLC.
;Status : Part Number:  Revision: 1.00
;==================
#Profibus_DP
;GSD_Revision=0

;General parameters
Vendor_Name = "Mettler-Toledo, LLC.      "
Model_Name = "IND570"
Revision = "1.00   "
Ident_number = 0x0EDA
Protocol_Ident = 0
Station_Type=0
FMS_supp = 0
Hardware_Release = "V 1.0  "
Software_Release = "1.00"
Bitmap_Device="T570EDA"
9.6_supp = 1
19.2_supp = 1
45.45_supp=1
93.75_supp = 1
187.5_supp = 1
500_supp = 1
1.5M_supp = 1
3M_supp = 1
6M_supp = 1
12M_supp = 1
MaxTsdr_9.6 = 60
MaxTsdr_19.2 = 60
MaxTsdr_45.45 = 60
MaxTsdr_93.75 = 60
MaxTsdr_187.5 = 60
MaxTsdr_500 = 100
MaxTsdr_1.5M = 150
MaxTsdr_3M = 250
MaxTsdr_6M = 450
MaxTsdr_12M = 800
Redundancy = 0
Repeater_Ctrl_Sig = 1
24V_Pins = 0
; Slave-Specification:
Freeze_Mode_supp = 0
Sync_Mode_supp = 0
Auto_Baud_supp = 1
Set_Slave_Add_supp = 0
User_Prm_Data_Len = 0x00
Min_Slave_Intervall = 2
Modular_Station = 1


Max_Module = 0x01
Max_Input_Len = 0x38
Max_Output_Len = 0x38
Max_Data_Len = 0x0070
Module= "I/O 2 Wrd" 0x61,0x51
EndModule
Module= "I/O 4 Wrd" 0x63,0x53
EndModule
Module= "I/O 6 Wrd" 0x65,0x55
EndModule
Module= "I/O 8 Wrd" 0x67,0x57
EndModule
Module= "I/O 12 Wrd" 0x6b,0x5b
EndModule
Module= "I/O 16 Wrd" 0x6f,0x5f
EndModule
Module= "I/O 17 Wrd" 0x6f,0x60,0x5f,0x50
EndModule
Module= "I/O 19 Wrd" 0x6f,0x62,0x5f,0x52
EndModule
Module= "I/O 21 Wrd" 0x6f,0x64,0x5f,0x54
EndModule
Module= "I/O 22 Wrd" 0x6f,0x65,0x5f,0x55
EndModule
Module= "I/O 23 Wrd" 0x6f,0x66,0x5f,0x56
EndModule
Module= "I/O 25 Wrd" 0x6f,0x68,0x5f,0x58
EndModule
Module= "I/O 28 Wrd" 0x6f,0x6b,0x5f,0x5b
EndModule
